Tevatron Upgrades:

• Commissioning of the Main Injector.

• Beam Energy: 1000 TeV ( √ s = 2.0 TeV) σ(pp̄ → tt̄) ↑ 40% • Luminosity: 2 ×10^{32} cm^{−2}s^{−1}

(×10 increase)

• Beam Crossings: 3.5 μsec → 396 nsec → 132 nsec • Delivered Luminosity: ≈ 2 fb^{−1} → 30 fb^{−1} (2 fb^{−1} is ×20 increase)