Detector Upgrades – CDF:

• Complete replacement of the central tracking systems.

{ New central drift chamber { New Silicon Vertex Detector (5 Layers Double Sided) ∗ 2x as long to cover most of luminous region ∗ 3-D Tracking (Stereo Strips) { Intermediate Silicon Tracking (w/ SVX, good ID to small ang.)

• New data aquisition system, trigger system, Frontend Elec. • Replacement of the calorimeters in the forward/backward direction.

• Upgrade to the muon detection system. (Greater coverage)