R. A. Briere Tracking with Helium 10

’

&

       $

       %

CLEO Data with DR2 Chamber

CLEO Drift Chamber ‘DR2’ • 40 Axial + 11 Stereo + 2 Cathodes C • [10 × (AAAS)] • 5A • S • 5A • C • 3:1 square cell • Max. drift: 7 mm • Isolated Stereo Layers

CLEOII Running: • 1989-95; 5 fb�^1 • DR2 with 50-50 Ar-C_2H_6 • Two other inner wire chambers: 6 + 10 axial layers

CLEO2.5 Running: • 1995-98; >5 fb�^1 • DR2 with 60-40 He-C_3H_8 • One other inner wire chambers: 10 axial layers • 3 layers double-sided Silicon

Compare CLEOII and CLEO2.5: Same chamber, different gas

Heavy Flavors ’97 Santa Barbara