R. A. Briere Tracking with Helium 11

’

&

       $

       %

CLEO DR2 Calibration

Basic Calibration T_0 Time Offset:

• Prompt timing edge (by channel) • Largely decoupled from D(T ) Drift Function D(T ):

• Mean of track projection in time bins for outer cell • Time integration for inner cell • Match at some fixed time. • Axial: One D(T ) • Stereo: separate D(T ) for left/right sides; as function of Z Corrections Entrance Angle Corrections (non-circular cells): • Calculated corrections (GARFIELD) • Stereo layer effects partly absorbed into fancier D(T ). Pulse-height corrections (time-slewing)

Heavy Flavors ’97 Santa Barbara