R. A. Briere Tracking with Helium 28

’

&

       $

       %

Summary of New Chambers

BaBar:

• Shortest (radial) chamber, low mass • No cathodes, most Silicon • Flat endplates, Be inner cylinder • Decoupled super-layers • Flattened hex cell

Belle:

• 3 inner cathodes (use in trigger); fewest stereo • Thinnest endplates • CFRP cylinders • Large radial dip at stereo super-layer edge

CLEO3:

• Evolution of existing design with subtle tweaks • 1 outer cathode for PID pointing • Thinnest inner cylinder • Smaller stereo angle, but more layers

Heavy Flavors ’97 Santa Barbara